 SE3000履带式液压挖掘机技术参数

Hydraulic Crawler Excavator Technical Specifications
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      发动机Engine
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    行走系统Travel System

	型号Model
	Weichai 16M33(Tier 3)
	行走总成Travel assembly
	川崎马达      KPM travel motor M3B1000BC

+南高齿减速机（NGC reducer）

	形式Type
	电控高压共轨、水冷、V型16缸、涡轮增压Electrical control,High-pressure common rail,water-cooling,16Cylinder with V-type,Turbocharging
	支重轮数量Support roller quantities
	9×2

	
	
	拖链轮数量Carrier roller quantities
	3×2

	缸数No. of cylinder
	16
	履带板数量Travel shoes （700mm）
	50×2

	缸径×行程Bore and stroke
	150mm×185mm
	行走速度Travel speed
	2.2/1.5km/h

	排量Displacement
	52.3L
	牵引力Drawbar pulling force
	1446

	额定功率Power output
	1468kW/1800rpm
	爬坡能力Grade ability
	70%(35°)

	
	
	配重离地间隙Ground clearance
	2277mm

	[image: image3.png]


    液压系统Hydraulic System
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   回转系统Swing System

	液压泵Main Pump
	川崎KPM K7V280
	回转马达Swing motor
	柱塞马达                Piston motor

	形式Type
	柱塞泵加齿轮泵

 piston pump plus gear pump 
	回转马达型号Swing motor type
	2×川崎KPM MX750

	额定工作流量

Max. discharge flow
	4x410+2x460L/min
	回转速度Swing speed
	3.8r/min

	主阀Main Valve
	KYB C0045( 3x750L/min)  
	回转减速机Swing reducer
	南高齿NGC
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  挖掘力Digging Force (ISO6015)
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      润滑油及容量

Refilling Capacities＆lubrication

	动臂长度 Boom length
	6570mm
	燃油箱容量Fuel tank
	5200L

	斗杆长度 Arm length
	4600mm
	冷却系统Cooling system
	420L

	铲斗挖掘力Bucket digging force
	978kN
	发动机机油量Engine oil
	230L

	斗杆挖掘力Arm digging force
	1016kN
	液压油箱Hydraulic oil tank
	1670L

	
	
	系统容量Hydraulic System 
	3200L
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      铲斗Bucket
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    操作重量和接地比压
Operating Weight and Ground Pressure

	型式Type
	Loading Shovel
	履带板宽度Shoe width
	1000mm

	铲斗容量Bucket capacity
	15.5m³
	接地比压Ground pressure
	201kPa

	铲斗宽度Bucket width
	3820mm
	操作重量Operating weight
	约Estimated:290000Kg

	工作范围Scope of work   (mm)
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	A
	最大挖掘高度Max. digging height
	15086
	

	B
	最大卸载高度Max. dumping height
	10386
	

	C
	最大挖掘深度Max. digging depth
	3727
	

	D
	最小挖掘距离
Min. digging distance
	5386
	

	E
	最小地面挖掘距离
Min. ground level digging distance
	8019
	

	F
	地面平推距离Push distance at ground level
	4995
	

	G
	最大卸载高度时的挖掘半径

Excavation radius at Max. dumping height
	8172
	

	H
	铲斗最大开口

Max. bucket opening
	2160
	

	外形尺寸 Dimensions    (mm)

	A
	总长Overall length
	17649
	I
	轮距Tread
	6335

	B
	接地长度（运输时）

Ground contact length (Transportation)
	14404
	J
	履带长度Track length
	8092

	C
	总高（至动臂顶部）

Overall height(to top of boom)
	7924
	K
	轨距Track gauge
	5000

	D
	总宽Overall width
	7858
	L
	底盘宽度Track width
	6640

	E
	总高（至驾驶室顶部）

Overall height(to top of cab)
	7536
	M
	履带板宽度Shoe width
	1000

	F
	配重离地间隙

Counter weight ground clearance
	2277
	N
	尾部高度Bonnet height
	4702

	G
	最小离地间隙Ground clearance
	785
	H2
	转台宽度Revolving frame width
	3500

	H
	尾部回转半径Tail swing radius
	6806
	Q
	回转中心至后端部距离

Distance from swivel center to tail
	6485
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